
R10945004


孫欽鉉

(1) Design a Mini-max lowpass FIR filter such that

(a) the frequency response



(b) the impulse response h[n]



(c) the maximal error for each iteration

